GVC1-Prime and GVC2-Prime Software Update Instructions

Getting the New Software – Updated 4/10/25
Software Download Link for GVC1 Prime 9383 (Blue control board): 
https://drive.google.com/file/d/1iq10RWywA5icQqFrHoeTnvCCUNpLQbiy/view?usp=sharing			
Software Download Link for GVC2 Prime 13150 (Red control board): 
https://drive.google.com/file/d/1eXj8UjMnhrVFDIq5-GFnXuu7AjK-bUiU/view?usp=sharing		
	· From the download links above choose either GVC1 Prime or GVC2 Prime based on your control board type.
· Download and save the file either to your Desktop or to your Downloads folder.
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	· Locate the downloaded file
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	· Rename the file to extension from “.bi_” to “.bin”
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	· Save the file to a USB drive
· The file must Not be in a folder. (the root)
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Programming the control board
Parts Needed
· USB Drive with software
· Jumper or coin to short programming pins

	· Using the machines power switch turn the power off 

· Locate USB port in the center of the control board
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	· Insert USB Drive in Port
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	· Locate Programming Pins next to USB port. 
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	· Use jumper or a coin to short the Programming Pins together. 
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	· With the jumper (or coin) still on the programming pins turn the power on to the machine.
· In the upper left-hand corner of the control board a light will rapidly flash while the board is programming. 
· If the light flashes slowly, your USB drive is not compatible. Try a different USB drive.
· When the light has stopped flashing, programming is complete, turn the machine power off
· Remove USB drive and jumper or coin. 
· Turn power on

· NOTE: Once you have programmed the control board, all setting returned to the factory default settings.
· Be sure to do a motor count, set prices and any other settings your machine may need such as, refrigeration, space to sales, etc. 
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Link to video of programming process:
https://www.dropbox.com/s/zpfx9v888rz10yv/20210128_165703000_iOS.mp4?dl=0 
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